POST LAB

module FS(diff, borr, a, b, c);

output diff;

output borr;

input a;

input b;

input c;

assign diff = a^b^c;

assign borr = c&(a^b)|(~a&b);

endmodule

FULL SUBTRACTOR OUTPUT WAVEFORM USING XILINX

